Specifications for Hamilton AM1000 AM transmitter

                             Fully legal, certified under Part 15 FCC

Power out    100 milliwatts

Frequency    1200Khz – 1720 Khz crystal controlled

Stability          50 PPM

Harmonics            -20DB Min

Audio In     600 OHM (TELEPHONE LINE)

AF response      20 Hz – 20 Khz

Size      8.5” x 4.75” x 3.5”

Power     12 VDC – 16 VDC Wall trans. Supplied

                                Volt Ohm Meter required for tune up
                                 
                                               Audio Response